



MayoStride Innovations

S.J Carew – EN1040

230 Elizabeth Ave, St. Johns

NL A1C 5S7

Canada

|  |  |
| --- | --- |
| **Product Specifications** | |
| **Product #: 000 002** | Heavy Duty Commercial  Emergency Light |
| Input | 120VAC 60Hz |
| Converters | 120VAC to 22VDC  5VDC |
| Battery | 12V TY-12-7.5 Tysonic Lead Acid Battery |
| Protection | 2A Fuse |
| Light | NOMA 12V 7W |
| Max Operation Length | 13 Hours |
| µController | Microchip PIC16F684 |
| Sensors | LDR 20-60kΩ |
| Indicators | 4x 5mm LEDs |
| Mounting | VESA Mount |
| Dimensions | 200x156x170mm(LxWxH) |
| Weight | 600g |

Reset

Test

120VAC

5VDC

Battery Low

Battery Charging